**Evaluation Schedule – Park Signage**

Tenderer 8

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Photographic Evidence** | **Durability, Reliability and general wear & tear** | **The visual and structural impact the sign** | **The orientation of the site and how the 3D maps work** | | **Price** | | **Max Total**  **100%** |
| Weighting | 20 | 20 | 10 | 10 | | 50 | |  |
| Base Points | 0 – 5 | 0 - 5 | 0 – 5 | 0 - 5 | | By simple ratio | |  |
| Maximum | 100 | 100 | 50 | 50 | | 200 | | 500 |
|  | Quality 60% | | | | | Price 40% | |  |
| Tenderers Name | The Art Department (TAD) | | | | | | |  |
| Photographic Evidence | Examples of flat and tray panel signs, totems, display case, map panels, welcome signage, interpretation panels with examples of parks environments. | | | | | | | 100 |
| Durability, Reliability and general wear & tear | Method statement conforms with specification requirements on:   * Materials quality * Eco paints for external environment offering prolonged UV resistance * 10 year vinyl with PVDF grade anti graffiti over laminate * Stainless steel anti vandal fixings | | | | | | | 100 |
| The visual and structural impact the sign | Based on method statement and examples of sites contained in photographic pack. Mock templates of how LCC contract requirements would work.  Site survey, true life mocks suggesting size, shape and spatial occupancy in a location specific sign guide. | | | | | | | 50 |
| The orientation of the site and how the 3D maps work | Eagle I 3D map details provide.  Examples provided. | | | | | | | 50 |
| Price | £41,993.00 | | | |  | | Points | 101 |
|  |  | | | | | | Total | 401 |